EUROGAM SUPPRESSION

J.Simpson

Shared suppression mode.

A possible mode of operation for the shared suppression in terms of which BGO detector suppresses which Ge detector is given below.

Ge detector BGO elements in the suppression No of BGOs 1 1a-1j,2f,2g,2h,6a,6e,5c,5d,5e,35a,35b,7i,7j 22 2 2a-2j,3f,3g,3h,6a,6b,1c,1d,1e,11a,11b,13i,13j 22 3 3a-3j,4f,4g,4h,6b,6c,2c,2d,2e,17a,17b,19i,19j 22 4 4a-4j,5f,5g,5h,6c,6d,3c,3d,3e,23a,23b,25i,25j 22 5 5a-5j,1f,1g,1h,6d,6e,4c,4d,4e,29a,29b,31i,31j 22 7 7a-7j,8f,8g,8h,12e,12a,11c,11d,11e,1a,1b,35i,35j 22 8 8a-8j,9f,9g,9h,12a,12b,7c,7d,7e,34a,34b,37i,37j 22 9 9a-9j,10f,10g,10h,12b,12c,8c,8d,8e,39a,39b,42i,42j 22 10 10a-10j,11f,11g,11h,12c,12d,9c,9d,9e,41a,41b,14i,14j 22 11 11a-11j,7f,7g,7h,12d,12e,10c,10d,10e,13a,13b,2i,2j 22 12 12a-12e,7e,7f,8e,8f,9e,9f,10e,10f,11e,11f 15 13 13a-13j,14f,14g,14h,18e,18a,17c,17d,17e,2a,2b,11i,11j 22 14 14a-14j,15f,15g,15h,18a,18b,13c,13d,13e,10a,10b,41i,41j 22 15 15a-15j,16f,16g,16h,18b,18c,14c,14d,14e,43a,43b,46i,46j 22 16 16a-16j,17f,17g,17h,18c,18d,15c,15d,15e,45a,45b,20i,20j 22 17 17a-17j,13f,13g,13h,18d,18e,16c,16d,16e,19a,19b,3i,3j 22 18 18a-18e,13e,13f,14e,14f,15e,15f,16e,16f,17e,17f 15 19 19a-19j,20f,20g,20h,24e,24a,23c,23d,23e,3a,3b,17i,17j 22 20 20a-20j,21f,21g,21h,24a,24b,19c,19d,19e,16a,16b,45i,45j 22 21 21a-21j,22f,22g,22h,24b,24c,20c,20d,20e,47a,47b,50i,50j 22 22 22a-22j,23f,23g,23h,24c,24d,21c,21d,21e,49a,49b,26i,26j 22 23 23a-23j,19f,19g,19h,24d,24e,22c,22d,22e,25a,25b,4i,4j 22 24 24a-24e,19e,19f,20e,20f,21e,21f,22e,22f,23e,23f 15 25 25a-25j,26f,26g,26h,30e,30a,29c,29d,29e,4a,4b,23i,23j 22 26 26a-26j,27f,27g,27h,30a,30b,25c,25d,25e,22a,22b,49i,49j 22 27 27a-27j,28f,28g,28h,30b,30c,26c,26d,26e,51a,51b,54i,54j 22 28 28a-28j,29f,29g,29h,30c,30d,27c,27d,27e,53a,53b,32i,32j 22 29 29a-29j,25f,25g,25h,30d,30e,28c,28d,28e,31a,31b,5i,5j 22 30 30a-30e,25e,25f,26e,26f,27e,27f,28e,28f,29e,29f 15 31 31a-31j,32f,32g,32h,36e,36a,35c,35d,35e,5a,5b,29i,29j 22 32 32a-32j,33f,33g,33h,36a,36b,31c,31d,31e,28a,28b,53i,53j 22 33 33a-33j,34f,34g,34h,36b,36c,32c,32d,32e,55a,55b,38i,38j 22 34 34a-34j,35f,35g,35h,36c,36d,33c,33d,33e,37a,37b,8i,8j 22 35 35a-35j,31f,31g,31h,36d,36e,34c,34d,34e,7a,7b,1i,1j 22 36 36a-36e,31e,31f,32e,32f,33e,33f,34e,34f,35e,35f 15

Ge detector BGO elements in the suppression No of BGOs 37 37a-37j,38f,38g,38h,41c,41d,41e,8a,8b,34i,34j 20 38 38a-38j,37c,37d,37e,33a,33b,65i,65j 17 41 41a-41j,37f,37g,37h,44a,44b,6i,6j 17 43 43a-43j,44f,44g,44h,47c,47d,47e,14a,14b,10i,10j 20 44 44a-44j,43c,43d,43e,9a,9b,41i,41j 17 47 47a-47j,43f,43g,43h,50a,50b,15i,15j 17 49 49a-49j,50f,50g,50h,53c,53d,53e,20a,20b,16i,16j 20 50 50a-50j,49c,49d,49e,15a,15b,47i,47j 17 53 53a-53j,49f,49g,49h,56a,56b,21i,21j 17 55 55a-55j,56f,56g,56h,59c,59d,59e,26a,26b,22i,22j 20 56 56a-56j,55c,55d,55e,21a,21b,53i,53j 17 59 59a-59j,55f,55g,55h,62a,62b,27i,27j 17 61 61a-61j,62f,62g,62h,65c,65d,65e,32a,32b,28i,28j 20 62 62a-62j,61c,61d,61e,27a,27b,59i,59j 17 65 65a-65j,61f,61g,61h,38a,38b,33i,33j 17

GAMIC SUPPRESSION

Individual suppression.

A possible mode of operation for the individual suppression mode in terms of which BGO detector suppresses which Ge detector is given below.

Ge detector BGO elements in the suppression No of BGOs 1 1a-1j 10 2 2a-2j 10 3 3a-3j 10 4 4a-4j 10 5 5a-5j 10 etc for Ge detectors 7,8 9,10,11,13,14,15,16,17,19,20,21,22,23,25,26,27 28,29,31,32,33,34,35,37,38,41,43,44,47,49,50,53,55,56,59,61,62,65.

And.

Ge detector BGO elements in the suppression No of BGOs 12 12a-12e,7e,7f,8e,8f,9e,9f,10e,10f,11e,11f 15 18 18a-18e,13e,13f,14e,14f,15e,15f,16e,16f,17e,17f 15 24 24a-24e,19e,19f,20e,20f,21e,21f,22e,22f,23e,23f 15 30 30e-30e,25e,25f,26e,26f,27e,27f,28e,28f,29e,29f 15 36 36e,36e,31e,31f,32e,32f,33e,33f,34e,34f,35e,35f 15