DETECTOR POSITION NUMBERING SCHEME

The array has 72 detector positions (with No 6 for the beam in and number 72

for the beam out). The numbering for the six germanium detectors in each main

pentagon face starts with the upermost detector in the corner of the pentagon and

goes clockwise around the face and ends with the detector in the middle.

The num bering for the type 1 BGO detectors is clockwise alphabetical ‘a’ to ‘j’

with ‘a’ and ‘j’ nearest a corner of a main pentagon. The type 2 BGO detectors

around the central Ge detector are numbered ‘a’ to ‘e’ with ‘a’ and ‘e’ nearest the

lowe st num bered Ge detector.

J.Simpson.