DOC228

MIDAS

Register Definitions for the LeCroy 4518 Module

Edition 1.0

Jan 1996

Nuclear Physics Support Group

Central Laboratory of the Research Councils

Daresbury Laboratory

Registers for the LeCroy 4518 module

This document should be read in conjunction with the document EDOC210 which describes the Register Server implementation for CAMAC .

The LeCroy 4518 (previously 4418) is a Programmable Logic Delay/Fan-Out.

All register attributes include -c (crate address) and -n (station address)

Registers using the xCAMAC class of the CAMAC Register Server

Delay Settings write by f(16 ) a(x)

Load delay time setting (4 bits) for channel x using subaddress x.

lc4518#*.delay* attributes -a x -f 16 -w 16 -p wo -l 4 -b 0