DOC232

MIDAS

Register Definitions for the LeCroy 4516 module

Edition 1.0

Jan 1996

Nuclear Physics Support Group

Central Laboratory of the Research Councils

Daresbury Laboratory

Registers for the LeCroy 4516 module

This document should be read in conjunction with the document EDOC210 which describes the Register Server implementation for CAMAC .

This is an Programmable Logic Unit.

All register attributes include -c (crate address) and -n (station address)

Registers using the cCAMAC class of the CAMAC Register Server

These registers do not require data and have no initial value. However readregister operations may return Q and X as data.

Set C0 to AND write or read by f(26 ) a(0)

Sets all C0s to AND mode.

lc4516#*.C0toANDmode attributes -a 0 -f 26

Set C0 to OR write or read by f(24 ) a(0)

Sets all C0s to OR mode.

lc4516#*.C0toORmode attributes -a 0 -f 24

Set C1 to AND write or read by f(26 ) a(1)

Sets all C1s to AND mode.

lc4516#*.C1toANDmode attributes -a 1 -f 26

Set C1 to OR write or read by f(24 ) a(1)

Sets all C1s to OR mode.

lc4516#*.C1toORmode attributes -a 1 -f 24

Test C0 read by f(27 ) a(0)

Returns Q=1 if C0 switch is in AND mode.

lc4516#*.C0inANDmode attributes -a 0 -f 27

Test C1 read by f(27) a(1)

Returns Q=1 if C1 switch is in AND mode.

lc4516#*.C1inANDmode attributes -a 1 -f 27