SAROC

Logic Inspection Point

Analogue Inspection Point

SS DAC

32

8Ren-Out

16 MHz

Strobeout

Strobein

Data

Ren-in

ClusterBGO ChannelBlock diagram

� energy

Gated Integrator

TimingAmplifier

Single e-discr.

Baseline Control

GatedIntegrator TAC ADC DualADC

TimeDiscr.

Channel Control

Local Trigger

Sum Pattern

SD Sum Energy

SD Time

Convert

Clock

SD Energy

Pattern

Pattern Val

Start Conversion

19

19 19 OR19Tacs FTStartTAC

Reset 19 19Chan reset

Analogue Reset

Threshold

Vslsc 19 InputfromBGO

Vslsc

Vslsc Time

Energy

Gate

Sum Energy OR19Tacs

Vslsc

Veto(from anti-Compton logic)

TAC

Vslsc FT (stop) start

SD Sum Time

Reset(Inhibit)