SAROC

Shaping Amp and TFA

Dual ADC

CFD TAC Local Trigger

Dual ADC Input from pre-amp

Enable & VXI Go

Fast Trigger

Validation

Inhibit (detector busy)

4 MeV energy

20 MeV energy

End of flat top

TFA output

Direct CFD output

GateTAC

Peak hold& Convert

Convert

Logic Inspection Point

Analogue Inspection Point clock

datadata clock

PZ Adjust

Pileup/BLR Threshold

Time aligned CFD output

CFD output delay

CFD output width

CFD Threshold

Pre-pulsepileup Veto

RejectEnable

Test Pulser SS DAC 32

8Valack

Delayed ValPulse Ren-Out

16 MHz

Strobeout

Strobein

Data

Ren-in Convert

TACreset

Reset

FT samp

ValSamp ClusterGe ChannelBlock diagram

Ian Lazarus May 1994 andADCClockGen.